PROJECT DEVELOPMENT PHASE

SPRINT-2

|  |  |
| --- | --- |
| Date | 5 NOVEMBER 2022 |
| Team ID | PNT2022TMID26841 |
| Project Name | Project - Hazardous Area Monitoring for Industrial Plant powered by IoT |
| Maximum Marks | 4 Marks |

This is the file for ESP 32 modules which ill be used as the smart beacons to transmit the data from the industry to IBM cloud.

This will upload the following to IBM cloud

1. **Temperature in Fahrenheit**
2. **Humidity**
3. **Air Quality Percentage**

**CODE :**

#include <WiFi.h> #include <PubSubClient.h> #include <DHT.h> WiFiClient wifiClient; String data3;

#define DHTTYPE DHT11 #define DHTPIN 9

DHT dht(DHTPIN, DHTTYPE);

#define ORG "v6wg8x"

#define DEVICE\_TYPE "nodeMcu" #define DEVICE\_ID "NodeMCU" #define TOKEN "123456789"

#define speed 0.034

void callback(char\* topic, byte\* playload, unsigned int payloadLength);

char server[] = ORG ".messaging.internetofthings.ibmcloud.com"; char publishTopic[] = "iot-2/evt/Data/fmt/json";

char topic[] = "iot-2/cmd/test/fmt/String"; char authMethod[] = "use-token-auth"; char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

PubSubClient client(server, 1883, callback , wifiClient); void publishData();

String command; String data = "";

long duration; float dist;

void setup()

{

Serial.begin(115200); dht.begin(); wifiConnect(); mqttConnect();

}

void loop() {

publishData(); delay(500);

if (!client.loop()) { mqttConnect();

}

}

void wifiConnect() {

Serial.print("Connecting to "); Serial.print("Wifi"); WiFi.begin("SSID","Passord");

while (WiFi.status() != WL\_CONNECTED) { delay(500);

Serial.print(".");

}

Serial.print("WiFi connected, IP address: "); Serial.println(WiFi.localIP());

}

void mqttConnect() {

if (!client.connected()) {

Serial.print("Reconnecting MQTT client to "); Serial.println(server); while (!client.connect(clientId, authMethod, token)) { Serial.print(".");

delay(500);

}

initManagedDevice(); Serial.println();

}

}

void initManagedDevice() { if (client.subscribe(topic)) {

Serial.println("IBM subscribe to cmd OK");

} else {

Serial.println("subscribe to cmd FAILED");

}

}

void publishData()

{

int sensorValue = analogRead(34); //MQT 135 connected to GPIO 34 (Analog ADC1\_CH6) Serial.print("AirQua=");

Serial.print(sensorValue, DEC); Serial.println(" PPM");

float humid = dht.readHumidity();

float temp = dht.readTemperature(true); float airQty = sensorValue/4095;

String payload = "{\"Temperature\":"; payload += temp;

payload += "}";

if (client.publish(publishTopic, (char\*) payload.c\_str())) { Serial.println("Publish OK");

}

payload = "{\"Air Quality\":"; payload += airQty;

payload += "%}";

if (client.publish(publishTopic, (char\*) payload.c\_str())) { Serial.println("Publish OK");

}

}

void callback(char\* subscribeTopic, byte\* payload, unsigned int payloadLength) { Serial.print("callback invoked for topic:");

Serial.println(subscribeTopic);

for (int i = 0; i < payloadLength; i++) { dist += (char)payload[i];

}

Serial.println("data:" + data3); if (data3 == "lighton") {

Serial.println(data3);

}

data3 = "";

}

Footer