# DEVELOP A PYTHON SCRIPT

|  |  |
| --- | --- |
| **Team ID** | **PNT2022TMID26841** |
| **Project Name** | **Hazardous Area Monitoring For Industrial Plant Powered by IoT** |

import time import sys

import ibmiotf.application import ibmiotf.device import random

#Provide your IBM Watson Device Credentials organization = "t969x0"

deviceType = "NodeMCU" deviceId = "9798803723" authMethod = "token" authToken = "@Vli\_@GnxGS8M3v3Es"

# Initialize GPIO

def myCommandCallback(cmd):

print("Command received: %s" % cmd.data['command']) status=cmd.data['command']

if status=="lighton": print ("led is on")

elif status== "lightoff": print ("led is off")

else :

print ("please send proper command")

#print(cmd)

try:

deviceOptions = {"org": organization, "type": deviceType, "id": deviceId,

"auth-method": authMethod, "auth-token": authToken} deviceCli = ibmiotf.device.Client(deviceOptions) #..............................................

except Exception as e:

print("Caught exception connecting device: %s" % str(e)) sys.exit()

# Connect and send a datapoint "hello" with value "world" into the cloud as an event of type "greeting" 10 times

deviceCli.connect()

while True:

#Get Sensor Data from DHT11

temp=random.randint(90,100) Humid=random.randint(60,100)

data = { 'temp' : temp, 'Humid': Humid } #print data

def myOnPublishCallback():

print ("Published Temperature = %s C" % temp, "Humidity = %s %%" % Humid, "to IBM Watson")

success = deviceCli.publishEvent("IoTSensor", "json", data, qos=0, on\_publish=myOnPublishCallback)

if not success:

print("Not connected to IoTF") time.sleep(1)

deviceCli.commandCallback = myCommandCallback

# Disconnect the device and application from the cloud deviceCli.disconnect()

# OUTPUT:

